***********************************************************************************************************************************
How to install drivers for SR2MOD01 and SR2MOD02 modems in Windows Vista 32 bits and Windows 7 32 bits:

- in the configuration panel, select the modem option and telephony, than under the ‘modems’ tab, click on the “add” button
- tick the “my modem is not detected”, then click on the “next” button
- click on “disk provided”, then go to the modem drivers directory of ZelioSoft 2
- select Vista32
- select MultitechA.INF
- under the drop-down list, select:
	- “MultiTech MT5634SMI-V92” for SR2MOD01
	- “MultiTech Systems GSM_GPRS Wireless Modem” for SR2MOD02

- enter the modem properties, then modify the following parameters:
	- speed: 115200
	- 7 data bits
	- pair parity
	- 1 stop bit

************************************************************************************************************************************
How to install drivers for SR2MOD01 and SR2MOD02 modems in OS Windows prior to Vista:
- in the configuration panel, select the modem option and telephony, than under the ‘modems’ tab, click on the “add” button
- tick the “my modem is not detected”, then click on the “next” button
- in the default modems, select ‘modem standard 56000bps’
- enter the modem properties, then modify the following parameters:
	- speed: 115200
	- 7 data bits
	- pair parity
	- 1 stop bit

***********************************************************************************************************************************
